* Signal cable (orange one) ==> D9 on Arduino
* Power cable (red one) ==> 5v pin on Arduino
* Ground cable (black or brown one) ==> ground pin on Arduino